   7 Workstation: Windows NT with NetWare Client Services


Windows* NT* 4.0 and Novell NetWare client Services Driver Installation
notes
=======================================================================

Location of driver: \NWSERVER\E100B.LAN
                    \NWSERVER\OEMSETUP.INF


General Instructions for Novell NetWare* Client Services Under Windows
NT Using the ODI Server Driver
======================================================================

1  Install the Novell NetWare Client Services per the instructions
   provided by Novell.
   
   Note: If the NDIS driver for the PRO/100+ is installed and you want
         to us the NetWare 32 ODI LAN driver, remove the NDIS driver
         from NT before going to step 2.  Novell NetWare Client service
         can be run with the NDIS 3 driver.

2  Start Windows NT and log in as ADMINISTRATOR (or another valid user
   name).

3  Double click the Network icon in the Control Panel. The "Network
   Settings" screen appears.

4  Select the Adapter tab.

5  Click the Add button.

6  Click the Have Disk button.

7  Insert the Configuration and Drivers disk into your drive and 
   enter the pathname <drive>:\nwserver.  Click OK to continue.

8  When "ODI Intel PRO/100+ adapter for NetWare" appears,
   click OK.

9  After the files are copied, the default driver settings will be
   displayed (they'll be displayed with their defaults which in most
   cases is OK).  Click OK when correct.
   
   Note: Do not click on Advanced Settings.  See the section titled
   Advanced Setting below.

   Speed: Specifies the line speed of the adapter.
             0    =    Auto detect (default)
             10   =    10 Mbps
             100  =    100 Mbps
   

   ForceDuplex:

   Note: The PRO/100+ TX adapter supports full duplex at 10 and 100
         Mbps. The PRO/100B T4 adapter does not support full duplex at
         100 Mbps. It does at 10 Mbps.  
             0 = auto-negotiate (default)
             1 = half duplex
             2 = full duplex
      
      Note: If the adapter is set to half or full duplex, set the SPEED
            parameter to either 10 or 100. (see SPEED)

10 Restart Windows NT to complete the installation.


Advanced Settings
=================

Only select Advanced Settings if you want to use local Administration of
Addressing or use multiple PRO/100+ adapters. Entering
Advanced Setting requires that you know the slot number the adapter is
using.

1  To get to Advanced Setting from the Network Dialog box selected the
   Adapters tab and highlight the ODI PRO/100+ adapter
   and click Configure.

2  Click Advanced.

3  There are 2 advanced options, Node Address Override and Slot.

   Node Address Override: Use this option to provide your own unique
   node address for the adapter.  The node address is a 12-digit
   hexadecimal number; the second digit must be one of the following
   digits: 2, 6, A, E.

   SLOT: Select the slot number the adapter is in. Only necessary if
   multiple PRO/100+ adapter cards are being used.  Before clicking OK,
   you must enter a valid slot number.  To exit without saving a slot
   number, click Cancel.



* Third-party trademarks are the property of their respective owners.
