   5 LAN Server


LAN Server Installation Notes
=============================

Location of files:  \NDIS\E100B.OS2   (OS/2* driver)
                    \NDIS\E100BEO2.NIF
      
                         or
      
                    \NDIS\E100B.DOS   (DOS driver)
                    \NDIS\E100BEDS.NIF (DLR and LSP installation file)

NOTE: LAN Requester needs DOS 3.3 through 5, but if you're using DOS 6.0
      or higher, run SETVER.EXE prior to using the executable files 
      found on the DOS LAN Requester disks. See your DOS manual if you
      need help with SETVER.EXE.


Sample configuration file
-------------------------

PROTOCOL.INI (will include):

[E100B_NIF]
   DriverName = E100B$


General installation - LAN Server and OS/2 Requester (4.0 or 3.0)
-----------------------------------------------------------------

1  Run the MPTS utility with LAN Server 4.0 or OS/2 Requester 4.0 (Run
   the LAPS utility with LAN Server 3.0 or OS/2 Requester 3.0).

2  Click Install.

3  When prompted, insert the Configuration and Drivers disk in the
   drive, specify <drive>:\NDIS for driver location, and click OK.

4  When Install reads the E100BEO2.NIF, installation is complete. Click
   OK.  The adapter driver has been copied to your system.

5  Click Configure from the MPTS window.

6  At the Configure window, make sure the LAN adapters and protocols
   button is on and click CONFIGURE.

7  At the LAPS Configuration window, select the PRO/100+ adapter (OS/2
   driver: E100B.OS2) from the Network Adapters window.
   
   Click Add in the Network Adapter window to add the PRO/100+ PCI
   adapter to the current configuration.

8  Select your desired protocol(s) from the Protocol window and click
   Add to add the protocol(s) to the current configuration.

9  Click OK when you're done and follow the prompts to exit MPTS. Your
   CONFIG.SYS is automatically updated.
   
   Shut down and reset your system for the changes to take effect.


General installation under DOS (DOS LAN Services)
=================================================

NOTE: Due to a problem with the DLS installation utility, you need to
      complete the following steps before executing the installation of
      DLS:
   
      1  On DLS Diskette 1, make a directory off the root called NDIS.
      
      2  Copy the file E100B.DOS (from the \NDIS directory of the
         Configuration and Drivers disk) into this new directory \NDIS
         on DLS disk 1.

1  Run the DOS LAN Services installation program at the DOS workstation.
   Follow the prompts.

2  When presented with an adapter list, select Network card not shown in
   list below.

3  When prompted for the location of the OEMSETUP.INF file, insert the
   Configuration and Drivers disk in your drive and enter <drive>:\NDIS
   as the path.

4  Select the PRO/100+ adapter from the list.  Follow the prompts.

5  Enter your machine name, user name and domain name.

6  Set the options as you need; then highlight "The listed options are
   correct" and press Enter.

7  Accept the defaults on the next screen, highlight "The listed options
   are correct" and press Enter.

8  Set the Speed, Duplex mode, or Slot Device if needed. We recommend
   accepting the defaults. Then highlight "The listed options are
   correct" and press Enter.

9  You may be asked to insert DLS disks. Follow the prompts to complete
   the installation and restart your computer for changes to take 
   effect.


General Installation Under DOS: LAN Support Program (LSP)
=========================================================

1  Run DXMAID from the LAN Support Program disk.

2  Follow the prompts and instructions.

3  When prompted, insert the Configuration and Drivers disk and
   enter the pathname <drive>:\NDIS.

4  The default configuration is suitable for most environments.  We
   recommend accepting the defaults.

5  After the installation is complete, restart your computer for the
   changes to take effect.


General Installation Under DOS (DOS LAN Requester)
==================================================

1  Run the DOS LAN Requester installation program at the DOS
   workstation. Follow the prompts to configure your DOS LAN Requester
   as you require.

2  After the installation is complete, restart your computer for the
   changes to take effect.


Advanced Settings
=================
   
   SPEED (optional; parameters are [Auto / 10 / 100]): The parameter
      disables Auto-Speed Detect and causes the adapter to function at
      the speed indicated. If the FORCEDUPLEX parameter is assigned to
      either 1 or 2, the SPEED parameter is required because auto-speed
      sensing is disabled if the duplex mode is forced. Auto-negotiate
      devices cannot detect speed changes in this configuration until
      the driver is reloaded. [Example: SPEED=100]
    
   FORCEDUPLEX: Supports auto-negotiate, full and half duplex at 10 
      or 100 Mbps.

      This parameter disables auto-negotiate capability and forces the
      adapter to operate in half or full duplex mode. The SPEED 
      parameter must be specified and must be valid if the default of
      auto-negotiate is changed. Options for FORCEDUPLEX are Auto (for
      auto-negotiate), 1 (for half), 2 (for full). [Example: FORCEDUPLEX
      = 2]
   
   SLOT: (required for multiple adapters) This parameter is optional if
      only one adapter is present.  If it is specified but is incorrect,
      a message indicates that the value doesn't match the configuration
      but the driver finds the adapter and loads anyway.
   
      This parameter is required if more than one adapter is present in
      either one bus or multiple PCI buses of a system. The parameter
      tells the driver which adapter it controls. The SLOT number is the
      encoded value of the PCI adapter's device location. To determine
      the slot number, load the driver with only the DRIVERNAME
      parameter specified.  The driver reports all the slots that have
      PCI adapter(s) installed. You can determine which card is in which
      slot by using SETUP.EXE and matching the Ethernet addresses of the
      adapter to the device number specified in View Configuration.
      [Example: SLOT=0x1C]



*  Third-party trademarks are the property of their respective owners.



