   4 Using IBM LAN support for AS/400 and NetWare


Installing and Configuring the Adapter

Using IBM LAN Support for AS/400 and NetWare*
=============================================

Location of Driver:  \NDIS\E100B.DOS (for LANSUP)
Location of Driver:  \DOS\E100BODI.COM (for ODINSUP)


(Sample configuration files are included below.)


General instructions
--------------------

There are two ways to connect the PRO/100+ adapter simultaneously
to an IBM AS/400 (or other host based on DLC protocol) and
a Novell server:

- Using LANSUP.COM (NDIS-based) or
- Using ODINSUP.COM (ODI-based)

LANSUP.COM and ODINSUP.COM are Novell drivers included in VLMUPx.EXE
(where x is the number of the latest version). The files are available
on Novell's Support Web site.


Sample CONFIG.SYS file for LANSUP
---------------------------------

DEVICE = \LANMAN\PROTMAN.DOS    (version 1.1 or later )
DEVICE = \LANMAN\E100B.DOS      (version 1.34 or later)
DEVICE = \LANMAN\DXMA0MOD.SYS   (version 1.35 or later)
DEVICE = \LANMAN\DXME0MOD.SYS   (version 1.35 or later)
DEVICE = C:\PCS\EIMPCS.SYS
DEVICE = C:\PCS\ECYDDX.SYS


Sample AUTOEXEC.BAT file for LANSUP
-----------------------------------

CD\LANMAN
NETBIND                         (version 1.1 or later )
LSL                             (version 2.11 or later)
LANSUP                          (version 1.27 or later)
IPXODI                          (version 2.20 or later)
NETX or VLM                     (version 3.32 or later of
                                 NETX.EXE, or version 1.20
                                 or later of VLM.EXE)
F:
LOGIN
C:\PCS\STARTPCS


Sample PROTOCOL.INI file for LANSUP
-----------------------------------

[PROTOCOL MANAGER]
   DRIVERNAME = PROTMAN$

[ETHERNET]
   DRIVERNAME = DXME0$
   BINDINGS = E100B

[E100B]
   DRIVERNAME = E100B$


Sample NET.CFG file for LANSUP
------------------------------

Link Driver LANSUP
   Max Frame Size = 1490

NetWare DOS Requester
   First Network Drive = F


Sample CONFIG.SYS file for ODINSUP
----------------------------------

DEVICE = \LANMAN\PROTMAN.DOS /I:C:\LAMAN   (version 1.1 or later)
DEVICE = \LANMAN\DXMA0MOD.SYS              (version 1.35 or later)
DEVICE = \LANMAN\DXME0MOD.SYS              (version 1.35 or later)
DEVICE = C:\PCS\EIMPCS.SYS
DEVICE = C:\PCS\ECYDDX.SYS


Sample AUTOEXEC.BAT file for ODINSUP
------------------------------------

CD\LANMAN
LSL                                       (version 2.11 or later)
E100BODI                                  (version 1.25 or later)
ODINSUP                                   (version 2.00 or later)
NETBIND                                   (version 1.1 or later)
IPXODI                                    (version 2.20 or later)
NETX or VLM                    (version 3.32 or later of NETX.EXE;
                                version 1.20 or later of VLM.EXE)
F:
LOGIN
C:\PCS\STARTPCS


Sample PROTOCOL.INI file for ODINSUP
------------------------------------

[PROTOCOL MANAGER]
   DRIVERNAME = PROTMAN$

[ETHERNET]
   DRIVERNAME = DXME0$
   BINDINGS = E100BODI

[E100BODI]
   DRIVERNAME = E100BODI$


Sample NET.CFG (C:\LANMAN\NET.CFG) file for ODINSUP
---------------------------------------------------

Link Driver E100BODI
   Frame ethernet_802.2
   Frame ethernet_II
   Frame ethernet_802.2
   Frame ethernet_snap

Protocol ODINSUP
   Bind  E100BODI

NetWare DOS Requester
   First Network Drive = F



*  Third-party trademarks are the property of their respective owners.
