; NET82557.INF
; Version 1.81  (PC98PAK [Win98 Push] version)
; $Revision: 2 $
; Copyright 1998 Intel Corp.
;

[Version]
LayoutFile=layout.inf
Signature="$Windows NT$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%V_INTEL%
;;;For Windows NT 5, this must be removed, until an official catalog file is present
;;;CatalogFile = e100b.cat


[Manufacturer]
%V_INTEL%=INTEL


;----------------------------------------------------------------------------
; Device section
; 
[INTEL]
%PCIE100BTX.DeviceDesc%    =PCIE100BTX.ndi,PCI\VEN_8086&DEV_1229&SUBSYS_00018086
%PCIE100BT4.DeviceDesc%    =PCIE100BT4.ndi,PCI\VEN_8086&DEV_1229&SUBSYS_00028086
%PCIE10PPCI.DeviceDesc%    =PCIE10PPCI.ndi,PCI\VEN_8086&DEV_1229&SUBSYS_00038086
%PCIE100RWU.DeviceDesc%    =PCIE100RWU.ndi,PCI\VEN_8086&DEV_1229&SUBSYS_00048086
%I557IFE.DeviceDesc%       =I557IFE.ndi,PCI\VEN_8086&DEV_1229&SUBSYS_00058086
%I557IFEWFM.DeviceDesc%    =I557IFEWFM.ndi,PCI\VEN_8086&DEV_1229&SUBSYS_00068086
%I558IFE.DeviceDesc%       =I558IFE.ndi,PCI\VEN_8086&DEV_1229&SUBSYS_00078086
%I558IFEWFM.DeviceDesc%    =I558IFEWFM.ndi,PCI\VEN_8086&DEV_1229&SUBSYS_00088086
%PCIE100PLUS.DeviceDesc%   =PCIE100PLUS.ndi,PCI\VEN_8086&DEV_1229&SUBSYS_00098086
%PCIE100MAN.DeviceDesc%    =PCIE100MAN.ndi,PCI\VEN_8086&DEV_1229&SUBSYS_000A8086
%PCIE100SERVER.DeviceDesc% =PCIE100SERVER.ndi,PCI\VEN_8086&DEV_1229&SUBSYS_10098086
%PCIE100DUAL.DeviceDesc%   =PCIE100DUAL.ndi,PCI\VEN_8086&DEV_1229&SUBSYS_10F08086
%PCIE100B.DeviceDesc%      =PCIE100B.ndi,PCI\VEN_8086&DEV_1229&REV_01
%PCIE100B2.DeviceDesc%     =PCIE100B2.ndi,PCI\VEN_8086&DEV_1229&REV_02
%PCIE100B2.DeviceDesc%     =PCIE100B4.ndi,PCI\VEN_8086&DEV_1229&REV_04
%PCIE100B2.DeviceDesc%     =PCIE100B5.ndi,PCI\VEN_8086&DEV_1229&REV_05
%PCIE100B2.DeviceDesc%     =PCIE100B6.ndi,PCI\VEN_8086&DEV_1229&REV_06


;----------------------------------------------------------------------------
; Install sections
; 
[PCIE100B.ndi]
CopyFiles=PCIE100B.ndi.copyfiles,PCIE100B.inf.copyfiles
AddReg=PCIE100B.ndi.reg,E100B.ndi.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100B2.ndi]
CopyFiles=PCIE100B.ndi.copyfiles,PCIE100B.inf.copyfiles
AddReg=PCIE100B2.ndi.reg,E100B.ndi.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100B4.ndi]
CopyFiles=PCIE100B.ndi.copyfiles,PCIE100B.inf.copyfiles
AddReg=PCIE100B4.ndi.reg,E100B.ndi.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100B5.ndi]
CopyFiles=PCIE100B.ndi.copyfiles,PCIE100B.inf.copyfiles
AddReg=PCIE100B5.ndi.reg,E100B.ndi.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100B6.ndi]
CopyFiles=PCIE100B.ndi.copyfiles,PCIE100B.inf.copyfiles
AddReg=PCIE100B6.ndi.reg,E100B.ndi.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100BTX.ndi]
CopyFiles=PCIE100B.ndi.copyfiles,PCIE100B.inf.copyfiles
AddReg=PCIE100BTX.ndi.reg,E100B.ndi.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100BT4.ndi]
CopyFiles=PCIE100B.ndi.copyfiles,PCIE100B.inf.copyfiles
AddReg=PCIE100BT4.ndi.reg,E100B.ndi.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE10PPCI.ndi]
CopyFiles=PCIE100B.ndi.copyfiles,PCIE100B.inf.copyfiles
AddReg=PCIE10PPCI.ndi.reg,E100B.ndi.reg,E100B_10.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100RWU.ndi]
CopyFiles=PCIE100B.ndi.copyfiles,PCIE100B.inf.copyfiles
AddReg=PCIE100RWU.ndi.reg,E100B.ndi.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[I557IFE.ndi]
CopyFiles=PCIE100B.ndi.copyfiles,PCIE100B.inf.copyfiles
AddReg=I557IFE.ndi.reg,E100B.ndi.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[I557IFEWFM.ndi]
CopyFiles=PCIE100B.ndi.copyfiles,PCIE100B.inf.copyfiles
AddReg=I557IFEWFM.ndi.reg,E100B.ndi.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[I558IFE.ndi]
CopyFiles=PCIE100B.ndi.copyfiles,PCIE100B.inf.copyfiles
AddReg=I558IFE.ndi.reg,E100B.ndi.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[I558IFEWFM.ndi]
CopyFiles=PCIE100B.ndi.copyfiles,PCIE100B.inf.copyfiles
AddReg=I558IFEWFM.ndi.reg,E100B.ndi.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100PLUS.ndi]
CopyFiles=PCIE100B.ndi.copyfiles,PCIE100B.inf.copyfiles
AddReg=PCIE100PLUS.ndi.reg,E100B.ndi.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100MAN.ndi]
CopyFiles=PCIE100B.ndi.copyfiles,PCIE100B.inf.copyfiles
AddReg=PCIE100MAN.ndi.reg,E100B.ndi.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100SERVER.ndi]
CopyFiles=PCIE100B.ndi.copyfiles,PCIE100B.inf.copyfiles
AddReg=PCIE100SERVER.ndi.reg,E100B.ndi.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100DUAL.ndi]
CopyFiles=PCIE100B.ndi.copyfiles,PCIE100B.inf.copyfiles
AddReg=PCIE100DUAL.ndi.reg,E100B.ndi.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg


;;  NT 5.0 specific

[PCIE100B.ndi.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
CopyFiles=PCIE100B_NT.ndis5.copyfiles
AddReg=PCIE100B.ndi.reg,E100B.ndi.NT.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100B.ndi.NT.Services]
AddService = E100B, 2, e100b.Service, common.EventLog

[PCIE100B2.ndi.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
CopyFiles=PCIE100B_NT.ndis5.copyfiles
AddReg=PCIE100B2.ndi.reg,E100B.ndi.NT.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100B2.ndi.NT.Services]
AddService = E100B, 2, e100b.Service, common.EventLog

[PCIE100B4.ndi.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
CopyFiles=PCIE100B_NT.ndis5.copyfiles
AddReg=PCIE100B4.ndi.reg,E100B.ndi.NT.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100B4.ndi.NT.Services]
AddService = E100B, 2, e100b.Service, common.EventLog

[PCIE100B5.ndi.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
CopyFiles=PCIE100B_NT.ndis5.copyfiles
AddReg=PCIE100B5.ndi.reg,E100B.ndi.NT.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100B5.ndi.NT.Services]
AddService = E100B, 2, e100b.Service, common.EventLog

[PCIE100B6.ndi.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
CopyFiles=PCIE100B_NT.ndis5.copyfiles
AddReg=PCIE100B6.ndi.reg,E100B.ndi.NT.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100B6.ndi.NT.Services]
AddService = E100B, 2, e100b.Service, common.EventLog

[PCIE100BTX.ndi.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
CopyFiles=PCIE100B_NT.ndis5.copyfiles
AddReg=PCIE100BTX.ndi.reg,E100B.ndi.NT.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100BTX.ndi.NT.Services]
AddService = E100B, 2, e100b.Service, common.EventLog

[PCIE100BT4.ndi.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
CopyFiles=PCIE100B_NT.ndis5.copyfiles
AddReg=PCIE100BT4.ndi.reg,E100B.ndi.NT.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100BT4.ndi.NT.Services]
AddService = E100B, 2, e100b.Service, common.EventLog

[PCIE10PPCI.ndi.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
CopyFiles=PCIE100B_NT.ndis5.copyfiles
AddReg=PCIE10PPCI.ndi.reg,E100B.ndi.NT.reg,E100B_10.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE10PPCI.ndi.NT.Services]
AddService = E100B, 2, e100b.Service, common.EventLog

[PCIE100RWU.ndi.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
CopyFiles=PCIE100B_NT.ndis5.copyfiles
AddReg=PCIE100RWU.ndi.reg,E100B.ndi.NT.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100RWU.ndi.NT.Services]
AddService = E100B, 2, e100b.Service, common.EventLog

[I557IFE.ndi.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
CopyFiles=PCIE100B_NT.ndis5.copyfiles
AddReg=I557IFE.ndi.reg,E100B.ndi.NT.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[I557IFE.ndi.NT.Services]
AddService = E100B, 2, e100b.Service, common.EventLog

[I557IFEWFM.ndi.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
CopyFiles=PCIE100B_NT.ndis5.copyfiles
AddReg=I557IFEWFM.ndi.reg,E100B.ndi.NT.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[I557IFEWFM.ndi.NT.Services]
AddService = E100B, 2, e100b.Service, common.EventLog

[I558IFE.ndi.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
CopyFiles=PCIE100B_NT.ndis5.copyfiles
AddReg=I558IFE.ndi.reg,E100B.ndi.NT.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[I558IFE.ndi.NT.Services]
AddService = E100B, 2, e100b.Service, common.EventLog

[I558IFEWFM.ndi.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
CopyFiles=PCIE100B_NT.ndis5.copyfiles
AddReg=I558IFEWFM.ndi.reg,E100B.ndi.NT.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[I558IFEWFM.ndi.NT.Services]
AddService = E100B, 2, e100b.Service, common.EventLog

[PCIE100PLUS.ndi.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
CopyFiles=PCIE100B_NT.ndis5.copyfiles
AddReg=PCIE100PLUS.ndi.reg,E100B.ndi.NT.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100PLUS.ndi.NT.Services]
AddService = E100B, 2, e100b.Service, common.EventLog

[PCIE100MAN.ndi.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
CopyFiles=PCIE100B_NT.ndis5.copyfiles
AddReg=PCIE100MAN.ndi.reg,E100B.ndi.NT.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100MAN.ndi.NT.Services]
AddService = E100B, 2, e100b.Service, common.EventLog

[PCIE100SERVER.ndi.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
CopyFiles=PCIE100B_NT.ndis5.copyfiles
AddReg=PCIE100SERVER.ndi.reg,E100B.ndi.NT.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100SERVER.ndi.NT.Services]
AddService = E100B, 2, e100b.Service, common.EventLog

[PCIE100DUAL.ndi.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5    ; PCI
CopyFiles=PCIE100B_NT.ndis5.copyfiles
AddReg=PCIE100DUAL.ndi.reg,E100B.ndi.NT.reg,E100B_100.ndi.reg,E100B_GENERIC.ndi.reg

[PCIE100DUAL.ndi.NT.Services]
AddService = E100B, 2, e100b.Service, common.EventLog



;----------------------------------------------------------------------------
; Device registration
; 
[PCIE100B.ndi.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_8086&DEV_1229&REV_01"

[PCIE100B2.ndi.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_8086&DEV_1229&REV_02"

[PCIE100B4.ndi.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_8086&DEV_1229&REV_04"

[PCIE100B5.ndi.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_8086&DEV_1229&REV_05"

[PCIE100B6.ndi.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_8086&DEV_1229&REV_06"

[PCIE100BTX.ndi.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_8086&DEV_1229&SUBSYS_00018086"

[PCIE100BT4.ndi.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_8086&DEV_1229&SUBSYS_00028086"

[PCIE10PPCI.ndi.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_8086&DEV_1229&SUBSYS_00038086"

[PCIE100RWU.ndi.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_8086&DEV_1229&SUBSYS_00048086"

[I557IFE.ndi.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_8086&DEV_1229&SUBSYS_00058086"

[I557IFEWFM.ndi.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_8086&DEV_1229&SUBSYS_00068086"

[I558IFE.ndi.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_8086&DEV_1229&SUBSYS_00078086"

[I558IFEWFM.ndi.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_8086&DEV_1229&SUBSYS_00088086"

[PCIE100PLUS.ndi.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_8086&DEV_1229&SUBSYS_00098086"

[PCIE100MAN.ndi.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_8086&DEV_1229&SUBSYS_000A8086"

[PCIE100SERVER.ndi.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_8086&DEV_1229&SUBSYS_10098086"

[PCIE100DUAL.ndi.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_8086&DEV_1229&SUBSYS_10F08086"


;----------------------------------------------------------------------------
; Common NDI parameters
; 
[E100B_GENERIC.ndi.reg]
HKR,Ndi\Params\DriverName,ParamDesc,0,"Driver Name"
HKR,Ndi\Params\DriverName,Type,0,"edit"
HKR,Ndi\Params\DriverName,Default,0,"E100B$"
HKR,Ndi\Params\DriverName,Flag,1,10,00,00,00

HKR,Ndi\Params\MapRegisters,ParamDesc,0,"Map Registers"
HKR,Ndi\Params\MapRegisters,Type,0,"int"
HKR,Ndi\Params\MapRegisters,Default,0,"64"
HKR,Ndi\Params\MapRegisters,Flag,1,20,00,00,00
HKR,Ndi\Params\MapRegisters,Min,0,"0"
HKR,Ndi\Params\MapRegisters,Max,0,"64"
HKR,Ndi\Params\MapRegisters,Step,0,"1"
HKR,Ndi\Params\MapRegisters,Base,0,"10"

HKR,Ndi\Params\Eid,ParamDesc,0,"Ethernet ID"
HKR,Ndi\Params\Eid,Type,0,"dword"
HKR,Ndi\Params\Eid,Default,0,"0"
HKR,Ndi\Params\Eid,Flag,1,20,00,00,00
HKR,Ndi\Params\Eid,Base,0,"10"

HKR,Ndi\Params\NumRfd,ParamDesc,0,"Receive Frame Descriptors"
HKR,Ndi\Params\NumRfd,Type,0,"int"
HKR,Ndi\Params\NumRfd,Default,0,"32"
HKR,Ndi\Params\NumRfd,Flag,1,20,00,00,00
HKR,Ndi\Params\NumRfd,Min,0,"1"
HKR,Ndi\Params\NumRfd,Max,0,"00001024"
HKR,Ndi\Params\NumRfd,Step,0,"1"
HKR,Ndi\Params\NumRfd,Base,0,"10"

HKR,Ndi\Params\NumTcb,ParamDesc,0,"Transmit Control Blocks"
HKR,Ndi\Params\NumTcb,Type,0,"int"
HKR,Ndi\Params\NumTcb,Default,0,"16"
HKR,Ndi\Params\NumTcb,Flag,1,20,00,00,00
HKR,Ndi\Params\NumTcb,Min,0,"1"
HKR,Ndi\Params\NumTcb,Max,0,"00000064"
HKR,Ndi\Params\NumTcb,Step,0,"1"
HKR,Ndi\Params\NumTcb,Base,0,"10"

HKR,Ndi\Params\NumCoalesce,ParamDesc,0,"Coalesce Buffers"
HKR,Ndi\Params\NumCoalesce,Type,0,"int"
HKR,Ndi\Params\NumCoalesce,Default,0,"8"
HKR,Ndi\Params\NumCoalesce,Flag,1,20,00,00,00
HKR,Ndi\Params\NumCoalesce,Min,0,"1"
HKR,Ndi\Params\NumCoalesce,Max,0,"00000032"
HKR,Ndi\Params\NumCoalesce,Step,0,"1"
HKR,Ndi\Params\NumCoalesce,Base,0,"10"

HKR,Ndi\Params\Adaptive_IFS,ParamDesc,0,"Adaptive Inter-Frame Spacing"
HKR,Ndi\Params\Adaptive_IFS,Type,0,"int"
HKR,Ndi\Params\Adaptive_IFS,Default,0,"1"
HKR,Ndi\Params\Adaptive_IFS,Flag,1,20,00,00,00
HKR,Ndi\Params\Adaptive_IFS,Min,0,"0"
HKR,Ndi\Params\Adaptive_IFS,Max,0,"255"
HKR,Ndi\Params\Adaptive_IFS,Step,0,"1"
HKR,Ndi\Params\Adaptive_IFS,Base,0,"10"

HKR,Ndi\Params\UcodeSW,ParamDesc,0,"Adaptive Technology"
HKR,Ndi\Params\UcodeSW,Type,0,"enum"
HKR,Ndi\Params\UcodeSW,Default,0,"1"
HKR,Ndi\Params\UcodeSW,Flag,1,30,00,00,00
HKR,Ndi\Params\UcodeSW\Enum,1,0,"On"
HKR,Ndi\Params\UcodeSW\Enum,0,0,"Off"

HKR,Ndi\params\NetworkAddress,ParamDesc,,"Locally Administered Address"
HKR,Ndi\params\NetworkAddress,Type,,edit
HKR,Ndi\params\NetworkAddress,Default,,0
HKR,Ndi\params\NetworkAddress,Flag,1,20,00,00,00
HKR,Ndi\params\NetworkAddress,Base,,16

HKR,Ndi\Params\AcpiWol,ParamDesc,0,"ACPI Wake On LAN"
HKR,Ndi\Params\AcpiWol,Type,0,"enum"
HKR,Ndi\Params\AcpiWol,Default,0,"1"
HKR,Ndi\Params\AcpiWol,Flag,1,20,00,00,00
HKR,Ndi\Params\AcpiWol\Enum,1,0,"Enabled"
HKR,Ndi\Params\AcpiWol\Enum,0,0,"Disabled"

HKLM,System\CurrentControlSet\Services\VxD\ACPIWOL,Start,1,00
HKLM,System\CurrentControlSet\Services\VxD\ACPIWOL,StaticVxD,0,"WOL558.vxd"

HKR,,MsPciScan,0,"2"


;----------------------------------------------------------------------------
; 100Mb only NDI parameters
; 
[E100B_100.ndi.reg]
HKR,Ndi\Params\Speed,ParamDesc,0,"Speed"
HKR,Ndi\Params\Speed,Type,0,"enum"
HKR,Ndi\Params\Speed,Default,0,"auto"
HKR,Ndi\Params\Speed,Flag,1,30,00,00,00
HKR,Ndi\Params\Speed\Enum,auto,0,"Automatic"
HKR,Ndi\Params\Speed\Enum,10,0,"10  Mb/sec"
HKR,Ndi\Params\Speed\Enum,100,0,"100 Mb/sec"

HKR,Ndi\Params\ForceDpx,ParamDesc,0,"Duplex Mode"
HKR,Ndi\Params\ForceDpx,Type,0,"enum"
HKR,Ndi\Params\ForceDpx,Default,0,"0"
HKR,Ndi\Params\ForceDpx,Flag,1,20,00,00,00
HKR,Ndi\Params\ForceDpx\Enum,0,0,"Auto Duplex Detect"
HKR,Ndi\Params\ForceDpx\Enum,1,0,"Half-Duplex"
HKR,Ndi\Params\ForceDpx\Enum,2,0,"Full-Duplex"


;----------------------------------------------------------------------------
; 10Mb only NDI parameters
; 
[E100B_10.ndi.reg]
HKR,Ndi\Params\ForceDpx,ParamDesc,0,"Duplex Mode"
HKR,Ndi\Params\ForceDpx,Type,0,"enum"
HKR,Ndi\Params\ForceDpx,Default,0,"1"
HKR,Ndi\Params\ForceDpx,Flag,1,20,00,00,00
HKR,Ndi\Params\ForceDpx\Enum,1,0,"Half-Duplex"
HKR,Ndi\Params\ForceDpx\Enum,2,0,"Full-Duplex"


;----------------------------------------------------------------------------
; NDI object registration
; 
[E100B.ndi.reg]
HKR,,DevLoader,0,"*ndis"
HKR,,DeviceVxDs,0,"e100bnt5.sys"
HKR,,EnumPropPages,0,"netdi.dll,EnumPropPages"
HKR,NDIS,LogDriverName,0,"E100B-100"
HKR,NDIS,MajorNdisVersion,1,03
HKR,NDIS,MinorNdisVersion,1,0A
HKR,NDIS\NDIS2,DriverName,0,"E100B$"
HKR,NDIS\NDIS2,FileName,0,"e100b.dos"
HKR,NDIS\ODI,DriverName,0,"e100bodi"
HKR,NDIS\ODI,FileName,0,"e100bodi.com"
HKR,Ndi,NdiInstaller,0,"8255xndi.dll,i557NdiProc"
HKR,Ndi\Interfaces,DefUpper,0,"ndis3,ndis2"
HKR,Ndi\Interfaces,DefLower,0,"ethernet"
HKR,Ndi\Interfaces,UpperRange,0,"ndis3,ndis2,odi"
HKR,Ndi\Interfaces,LowerRange,0,"ethernet"
HKR,Ndi\Install,ndis3,0,"E100B.ndis5"
HKR,Ndi\Install,ndis2,0,"E100B.ndis2"
HKR,Ndi\Install,odi,0,"E100B.odi"

; Uncomment the following line to enable INF for PC97 Certification
;HKR,Ndi\Install,ndis3,0,"E100B.ndis4.ff"

;----------------------------------------------------------------------------
; NT NDI object registration
; 
[E100B.ndi.NT.reg]
HKR,Ndi\Interfaces,            DefUpper,         0, "ndis5"
HKR,Ndi\Interfaces,            DefLower,         0, "ethernet"
HKR,Ndi\Interfaces,            UpperRange,       0, "ndis5"
HKR,Ndi\Interfaces,            LowerRange,       0, "ethernet"
HKR,Ndi,                       Service,          0, "E100B"


;----------------------------------------------------------------------------
; NT Service registration
; 
[e100b.Service]
DisplayName     = %e100bnt.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\e100bnt5.sys
LoadOrderGroup  = NDIS
AddReg          = TextModeFlags.reg


;-----------------------------------------------------------------------------
; NT Common base for all drivers for Eventlog and TextModeFlags
;
[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

[TextModeFlags.reg]
HKR, , TextModeFlags,    0x00010001, 0x0001


;----------------------------------------------------------------------------
; Driver Install Sections
; 
; Install NDIS5
[E100B.ndis5]
CopyFiles=E100B.ndis5.CopyFiles

; Install NDIS4
[E100B.ndis4]
CopyFiles=E100B.ndis4.CopyFiles

; Install NDIS4 (flat-file structure)
[E100B.ndis4.ff]
CopyFiles=E100B.ndis4.ff.CopyFiles

; Install NDIS3
[E100B.ndis3]
CopyFiles=E100B.ndis3.CopyFiles

; Install NDIS2
[E100B.ndis2]
CopyFiles=E100B.ndis2.CopyFiles

; Install ODI
[E100B.odi]
CopyFiles=E100B.odi.CopyFiles


;----------------------------------------------------------------------------
; Copy files
; 
[DestinationDirs]
DefaultDestDir=11
PCIE100B_NT.ndis5.CopyFiles  = 12
PCIE100B.inf.copyfiles=17
E100B.ndis2.CopyFiles=26
E100B.odi.CopyFiles=26

; Install NDI Installer Helper Dll
[PCIE100B.ndi.copyfiles]
8255xndi.dll,8255xndi.dl_,,2

[PCIE100B_NT.ndis5.copyfiles]
e100bnt5.sys,e100bnt5.sy_,,2

; Install INF
[PCIE100B.inf.copyfiles]
net82557.inf

[E100B.ndis4.CopyFiles]
e100bnt.sys,e100bnt.sy_,,2

[E100B.ndis5.CopyFiles]
e100bnt5.sys,e100bnt5.sy_,,2
WOL558.vxd,WOL558.vx_,,2

[E100B.ndis4.ff.CopyFiles]
e100bnt.sys,e100bnt.sy_,,2

[E100B.ndis3.CopyFiles]
e100b.sys,e100b.sy_,,2

[E100B.ndis2.CopyFiles]
e100b.dos,e100b.dos

[E100B.odi.CopyFiles]
e100bodi.com,e100bodi.com


;----------------------------------------------------------------------------
; Localizable Strings
; 
[Strings]
; Vendors
V_MS="Microsoft"
V_INTEL="Intel"

; Source disk name
DISKNAME="Adapter Configuration and Drivers Diskette"

; Device descriptions
PCIE100B.DeviceDesc="Intel EtherExpress PRO PCI Adapter"
PCIE100B2.DeviceDesc="Intel EtherExpress PRO PCI Adapter"
PCIE100BTX.DeviceDesc="Intel EtherExpress PRO/100B PCI Adapter (TX)"
PCIE100BT4.DeviceDesc="Intel EtherExpress PRO/100B PCI Adapter (T4)"
PCIE10PPCI.DeviceDesc="Intel EtherExpress PRO/10+ PCI Adapter"
PCIE100RWU.DeviceDesc="Intel EtherExpress PRO/100 WfM PCI Adapter"
I557IFE.DeviceDesc="Intel 82557-based Integrated Fast Ethernet"
I557IFEWFM.DeviceDesc="Intel 82557-based Integrated Fast Ethernet for WfM"
I558IFE.DeviceDesc="Intel 82558-based Integrated Fast Ethernet"
I558IFEWFM.DeviceDesc="Intel 82558-based Integrated Fast Ethernet for WfM"
PCIE100PLUS.DeviceDesc="Intel EtherExpress PRO/100+ PCI Adapter"
PCIE100MAN.DeviceDesc="Intel EtherExpress PRO/100+ Management Adapter"
PCIE100SERVER.DeviceDesc="Intel EtherExpress PRO/100+ Server Adapter"
PCIE100DUAL.DeviceDesc="Intel EtherExpress PRO/100+ Dual Port Adapter"
