--  Intelnic.mib version 4-1-1998

INTEL-NIC-MIB DEFINITIONS ::= BEGIN

IMPORTS
	enterprises
		FROM RFC1155-SMI
	nic-products
		FROM Intel-Common-MIB

	OBJECT-TYPE
		FROM RFC-1212
	Counter,Gauge,
	DisplayString
		FROM RFC1213-MIB;

DmiCounter			::= Counter
DmiCounter64		::= Counter64
DmiGauge			::= Gauge
DmiInteger			::= INTEGER
DmiOctetstring		::= OCTET STRING
DmiDisplaystring	::= DisplayString
DmiCompId	::= INTEGER
DmiGroupId	::= INTEGER
DmiDate	::= DisplayString 


intelnic        OBJECT IDENTIFIER ::= { nic-products    1 }


SintelComponentID ::= SEQUENCE {
	dManufacturerAtt1	DmiDisplaystring,
	productAtt2	DmiDisplaystring,
	versionAtt3	DmiDisplaystring,
	serialNumberAtt4	DmiDisplaystring,
	installationAtt5	DmiDate,
	verifyAtt6	DmiInteger
}

intelComponentIDTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF SintelComponentID
	ACCESS		not-accessible
	STATUS		mandatory
	DESCRIPTION	"This group defines the attributes common to all components.
This groupis required."
	::= {  intelnic 3 }

intelComponentIDEntry OBJECT-TYPE
	SYNTAX		SintelComponentID
	ACCESS		not-accessible
	STATUS		mandatory
	DESCRIPTION	"This group defines the attributes common to all components.
This groupis required."
	INDEX		{ DmiCompId,DmiGroupId }
	::= { intelComponentIDTable 1 }


dManufacturerAtt1 OBJECT-TYPE
	SYNTAX		DmiDisplaystring
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Manufacturer of this system."
	REFERENCE "'Intel|ComponentID|001' 1"
	::= { intelComponentIDEntry 1 }

productAtt2 OBJECT-TYPE
	SYNTAX		DmiDisplaystring
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Product name for this system."
	REFERENCE "'Intel|ComponentID|001' 2"
	::= { intelComponentIDEntry 2 }

versionAtt3 OBJECT-TYPE
	SYNTAX		DmiDisplaystring
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Version number of this system."
	REFERENCE "'Intel|ComponentID|001' 3"
	::= { intelComponentIDEntry 3 }

serialNumberAtt4 OBJECT-TYPE
	SYNTAX		DmiDisplaystring
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Serial number for this system."
	REFERENCE "'Intel|ComponentID|001' 4"
	::= { intelComponentIDEntry 4 }

installationAtt5 OBJECT-TYPE
	SYNTAX		DmiDate
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"The time and date when this component was installed."
	REFERENCE "'Intel|ComponentID|001' 5"
	::= { intelComponentIDEntry 5 }

verifyAtt6 OBJECT-TYPE
	SYNTAX		INTEGER {
		anErrorOccurredCheckStatusCode(0),
		thisComponentDoesNotExist(1),
		verificationIsNotSupported(2),
		reserved(3),
		thisComponentExistsButTheFunctionalityIsUntested(4),
		thisComponentExistsButTheFunctionalityIsUnknown(5),
		thisComponentExistsAndIsNotFunctioningCorrectly(6),
		thisComponentExistsAndIsFunctioningCorrectly(7)
	}
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"A code that provides a level of verification that the component is still installed and working."
	REFERENCE "'Intel|ComponentID|001' 6"
	::= { intelComponentIDEntry 6 }

SintelNetworkAdapterDriver ::= SEQUENCE {
	intelNetworkAdapterDriverState INTEGER,
	driverIndexAtt1	DmiInteger,
	driverSoftwareNameAtt2	DmiDisplaystring,
	driverSoftwareVersionAtt3	DmiDisplaystring,
	driverSoftwareDescriptionAtt4	DmiDisplaystring,
	driverSizeAtt5	DmiInteger,
	driverInterfaceTypeAtt6	DmiInteger,
	driverInterfaceVersionAtt7	DmiDisplaystring,
	driverInterfaceDescriptionAtt8	DmiDisplaystring
}

intelNetworkAdapterDriverTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF SintelNetworkAdapterDriver
	ACCESS		not-accessible
	STATUS		mandatory
	DESCRIPTION	""
	::= { intelnic  4 }

intelNetworkAdapterDriverEntry OBJECT-TYPE
	SYNTAX		SintelNetworkAdapterDriver
	ACCESS		not-accessible
	STATUS		mandatory
	DESCRIPTION	""
	INDEX		{ DmiCompId,DmiGroupId, driverIndexAtt1 }
	::= { intelNetworkAdapterDriverTable 1 }


intelNetworkAdapterDriverState OBJECT-TYPE
	SYNTAX		INTEGER {
		active(1),
		notInService(2),
		notReady(3),
		createAndGo(4),
		createAndWait(5),
		destroy(6)
	}
	ACCESS		read-write
	STATUS		mandatory
	REFERENCE "'Intel|Network Adapter Driver|001' 0"
	::= { intelNetworkAdapterDriverEntry 0 }

driverIndexAtt1 OBJECT-TYPE
	SYNTAX		DmiInteger
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	""
	REFERENCE "'Intel|Network Adapter Driver|001' 1"
	::= { intelNetworkAdapterDriverEntry 1 }

driverSoftwareNameAtt2 OBJECT-TYPE
	SYNTAX		DmiDisplaystring
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	""
	REFERENCE "'Intel|Network Adapter Driver|001' 2"
	::= { intelNetworkAdapterDriverEntry 2 }

driverSoftwareVersionAtt3 OBJECT-TYPE
	SYNTAX		DmiDisplaystring
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	""
	REFERENCE "'Intel|Network Adapter Driver|001' 3"
	::= { intelNetworkAdapterDriverEntry 3 }

driverSoftwareDescriptionAtt4 OBJECT-TYPE
	SYNTAX		DmiDisplaystring
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	""
	REFERENCE "'Intel|Network Adapter Driver|001' 4"
	::= { intelNetworkAdapterDriverEntry 4 }

driverSizeAtt5 OBJECT-TYPE
	SYNTAX		DmiInteger
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	""
	REFERENCE "'Intel|Network Adapter Driver|001' 5"
	::= { intelNetworkAdapterDriverEntry 5 }

driverInterfaceTypeAtt6 OBJECT-TYPE
	SYNTAX		INTEGER {
		other(1),
		ipx(2),
		odi(3),
		ndis(4),
		packetDriver(5),
		lantastic(6),
		unix(7),
		appletalk(8),
		ibmLanSupportProgram(9),
		llc(10),
		netbios(11),
		pathworksDLL(12)
	}
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Driver interface type."
	REFERENCE "'Intel|Network Adapter Driver|001' 6"
	::= { intelNetworkAdapterDriverEntry 6 }

driverInterfaceVersionAtt7 OBJECT-TYPE
	SYNTAX		DmiDisplaystring
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Driver interface version."
	REFERENCE "'Intel|Network Adapter Driver|001' 7"
	::= { intelNetworkAdapterDriverEntry 7 }

driverInterfaceDescriptionAtt8 OBJECT-TYPE
	SYNTAX		DmiDisplaystring
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Description of the driver interface."
	REFERENCE "'Intel|Network Adapter Driver|001' 8"
	::= { intelNetworkAdapterDriverEntry 8 }

SintelNetworkAdapter802Port ::= SEQUENCE {
	intelNetworkAdapter802PortState INTEGER,
	portIndexAtt1	DmiInteger,
	permanentNetworkAddressAtt2	DmiDisplaystring,
	currentNetworkAddressAtt3	DmiDisplaystring,
	connectorTypeAtt4	DmiInteger,
	dataRateAtt5	DmiInteger,
	totalPacketsTransmittedAtt6	DmiCounter64,
	totalBytesTransmittedAtt7	DmiCounter64,
	totalPacketsReceivedAtt8	DmiCounter64,
	totalBytesReceivedAtt9	DmiCounter64,
	totalTransmitErrorsAtt10	DmiCounter64,
	totalReceiveErrorsAtt11	DmiCounter64,
	totalHostErrorsAtt12	DmiCounter64,
	totalWireErrorsAtt13	DmiCounter64
}

intelNetworkAdapter802PortTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF SintelNetworkAdapter802Port
	ACCESS		not-accessible
	STATUS		mandatory
	DESCRIPTION	""
	::= { intelnic  5 }

intelNetworkAdapter802PortEntry OBJECT-TYPE
	SYNTAX		SintelNetworkAdapter802Port
	ACCESS		not-accessible
	STATUS		mandatory
	DESCRIPTION	""
	INDEX		{ DmiCompId,DmiGroupId, portIndexAtt1 }
	::= { intelNetworkAdapter802PortTable 1 }


intelNetworkAdapter802PortState OBJECT-TYPE
	SYNTAX		INTEGER {
		active(1),
		notInService(2),
		notReady(3),
		createAndGo(4),
		createAndWait(5),
		destroy(6)
	}
	ACCESS		read-write
	STATUS		mandatory
	REFERENCE "'Intel|Network Adapter 802 Port|001' 0"
	::= { intelNetworkAdapter802PortEntry 0 }

portIndexAtt1 OBJECT-TYPE
	SYNTAX		DmiInteger
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	" An index value that uniquely identifies the
           interface to an ethernet-like medium."
	REFERENCE "'Intel|Network Adapter 802 Port|001' 1"
	::= { intelNetworkAdapter802PortEntry 1 }

permanentNetworkAddressAtt2 OBJECT-TYPE
	SYNTAX		DmiDisplaystring

	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Permanent network address."
	REFERENCE "'Intel|Network Adapter 802 Port|001' 2"
	::= { intelNetworkAdapter802PortEntry 2 }

currentNetworkAddressAtt3 OBJECT-TYPE
	SYNTAX		DmiDisplaystring
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Current network address."
	REFERENCE "'Intel|Network Adapter 802 Port|001' 3"
	::= { intelNetworkAdapter802PortEntry 3 }

connectorTypeAtt4 OBJECT-TYPE
	SYNTAX		INTEGER {
		unknown(1),
		aUI(2),
		uTPCategory3(3),
		uTPCategory4(4),
		uTPCategory5(5),
		bNC(6),
		sTPRJ45(7),
		sTPDB9(8),
		fiberMIC(9),
		appleAUI(10)
	}
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Connector type."
	REFERENCE "'Intel|Network Adapter 802 Port|001' 4"
	::= { intelNetworkAdapter802PortEntry 4 }

dataRateAtt5 OBJECT-TYPE
	SYNTAX		DmiInteger
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Data rate."
	REFERENCE "'Intel|Network Adapter 802 Port|001' 5"
	::= { intelNetworkAdapter802PortEntry 5 }

totalPacketsTransmittedAtt6 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Total packets transmitted successfully."
	REFERENCE "'Intel|Network Adapter 802 Port|001' 6"
	::= { intelNetworkAdapter802PortEntry 6 }

totalBytesTransmittedAtt7 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Total bytes transmitted successfully."
	REFERENCE "'Intel|Network Adapter 802 Port|001' 7"
	::= { intelNetworkAdapter802PortEntry 7 }

totalPacketsReceivedAtt8 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Total packets received without errors."
	REFERENCE "'Intel|Network Adapter 802 Port|001' 8"
	::= { intelNetworkAdapter802PortEntry 8 }

totalBytesReceivedAtt9 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Total bytes received without errors."
	REFERENCE "'Intel|Network Adapter 802 Port|001' 9"
	::= { intelNetworkAdapter802PortEntry 9 }

totalTransmitErrorsAtt10 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Count of transmit errors."
	REFERENCE "'Intel|Network Adapter 802 Port|001' 10"
	::= { intelNetworkAdapter802PortEntry 10 }

totalReceiveErrorsAtt11 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Count of receive errors."
	REFERENCE "'Intel|Network Adapter 802 Port|001' 11"
	::= { intelNetworkAdapter802PortEntry 11 }

totalHostErrorsAtt12 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Count of host-side errors."
	REFERENCE "'Intel|Network Adapter 802 Port|001' 12"
	::= { intelNetworkAdapter802PortEntry 12 }

totalWireErrorsAtt13 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Count of network-side errors."
	REFERENCE "'Intel|Network Adapter 802 Port|001' 13"
	::= { intelNetworkAdapter802PortEntry 13 }

SintelNetworkAdapterInstrumentation ::= SEQUENCE {
	mIFIdAtt1	DmiInteger,
	versionAtt2	DmiDisplaystring
}

intelNetworkAdapterInstrumentationTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF SintelNetworkAdapterInstrumentation
	ACCESS		not-accessible
	STATUS		mandatory
	DESCRIPTION	""
	::= { intelnic  6 }

intelNetworkAdapterInstrumentationEntry OBJECT-TYPE
	SYNTAX		SintelNetworkAdapterInstrumentation
	ACCESS		not-accessible
	STATUS		mandatory
	DESCRIPTION	""
	INDEX		{ DmiCompId,DmiGroupId }
	::= { intelNetworkAdapterInstrumentationTable 1 }


mIFIdAtt1 OBJECT-TYPE
	SYNTAX		DmiInteger
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	""
	REFERENCE "'Intel|Network Adapter Instrumentation|001' 1"
	::= { intelNetworkAdapterInstrumentationEntry 1 }

versionAtt2 OBJECT-TYPE
	SYNTAX		DmiDisplaystring
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	""
	REFERENCE "'Intel|Network Adapter Instrumentation|001' 2"
	::= { intelNetworkAdapterInstrumentationEntry 2 }

SintelDriverExtensionsGroup ::= SEQUENCE {
	intelDriverExtensionsGroupState INTEGER,
	driverIndexAtt1	DmiInteger,
	driverFilePathAtt1	DmiDisplaystring,
	driverFileDateAtt2	DmiDisplaystring
}

intelDriverExtensionsGroupTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF SintelDriverExtensionsGroup
	ACCESS		not-accessible
	STATUS		mandatory
	DESCRIPTION	""
	::= { intelnic 7 }

intelDriverExtensionsGroupEntry OBJECT-TYPE
	SYNTAX		SintelDriverExtensionsGroup
	ACCESS		not-accessible
	STATUS		mandatory
	DESCRIPTION	""
	INDEX		{ DmiCompId,DmiGroupId, driverIndexAtt1 }
	::= { intelDriverExtensionsGroupTable 1 }


intelDriverExtensionsGroupState OBJECT-TYPE
	SYNTAX		INTEGER {
		active(1),
		notInService(2),
		notReady(3),
		createAndGo(4),
		createAndWait(5),
		destroy(6)
	}
	ACCESS		read-write
	STATUS		mandatory
	REFERENCE "'Intel|Network Adapter Driver Extensions Group|001' 0"
	::= { intelDriverExtensionsGroupEntry 0 }

driverIndexAtt1 OBJECT-TYPE
	SYNTAX		DmiInteger
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	" An index value that uniquely identifies the
           interface to an ethernet-like medium."
	REFERENCE "'Intel|Network Adapter Driver Extensions Group|001' 1"

	::= { intelDriverExtensionsGroupEntry 1 }

driverFilePathAtt1 OBJECT-TYPE
	SYNTAX		DmiDisplaystring
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"The file path of the adapter driver."
	REFERENCE "'Intel|Network Adapter Driver Extensions Group|001' 2"
	::= { intelDriverExtensionsGroupEntry 2 }

driverFileDateAtt2 OBJECT-TYPE
	SYNTAX		DmiDisplaystring
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"Adapter driver file date."
	REFERENCE "'Intel|Network Adapter Driver Extensions Group|001' 3"
	::= { intelDriverExtensionsGroupEntry 3 }

SintelEtherLike ::= SEQUENCE {
	intelEtherLikeState INTEGER,
	indexAtt1	DmiInteger,
	alignmentErrorsAtt2	DmiCounter64,
	fcsErrorsAtt3	DmiCounter64,
	singleCollisionFramesAtt4	DmiCounter64,
	multipleCollisionFramesAtt5	DmiCounter64,
	sqeTestErrorsAtt6	DmiCounter64,
	deferredTransmissionsAtt7	DmiCounter64,
	lateCollisionsAtt8	DmiCounter64,
	excessiveCollisionsAtt9	DmiCounter64,
	internalMacTransmitErrorsAtt10	DmiCounter64,
	carrierSenseErrorsAtt11	DmiCounter64,
	frameTooLongAtt12	DmiCounter64,
	internalMacReceiveErrorsAtt13	DmiCounter64,
	etherChipSetAtt14	DmiDisplaystring
}

intelEtherLikeTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF SintelEtherLike
	ACCESS		not-accessible
	STATUS		mandatory
	DESCRIPTION	""
	::= { intelnic  8 }

intelEtherLikeEntry OBJECT-TYPE
	SYNTAX		SintelEtherLike
	ACCESS		not-accessible
	STATUS		mandatory
	DESCRIPTION	""
	INDEX		{ DmiCompId,DmiGroupId, indexAtt1 }
	::= { intelEtherLikeTable 1 }


intelEtherLikeState OBJECT-TYPE
	SYNTAX		INTEGER {
		active(1),
		notInService(2),
		notReady(3),
		createAndGo(4),
		createAndWait(5),
		destroy(6)
	}
	ACCESS		read-write
	STATUS		mandatory
	REFERENCE "'Intel|Ether-like|001' 0"
	::= { intelEtherLikeEntry 0 }

indexAtt1 OBJECT-TYPE
	SYNTAX		DmiInteger
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"An index value that uniquely identifies the
           interface to an ethernet-like medium."
	REFERENCE "'Intel|Ether-like|001' 1"
	::= { intelEtherLikeEntry 1 }

alignmentErrorsAtt2 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"A count of frames received on a particular 
               interface that are not an integral number of
               octets in length and do not pass the FCS check."
	REFERENCE "'Intel|Ether-like|001' 2"
	::= { intelEtherLikeEntry 2 }

fcsErrorsAtt3 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"A count of frames received on a particular
         interface that are an integral number of octets
         in length but do not pass the FCS check."
	REFERENCE "'Intel|Ether-like|001' 3"
	::= { intelEtherLikeEntry 3 }


singleCollisionFramesAtt4 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"A count of successfully transmitted frames on
         a particular interface for which transmission
         is inhibited by exactly one collision."
	REFERENCE "'Intel|Ether-like|001' 4"
	::= { intelEtherLikeEntry 4 }

multipleCollisionFramesAtt5 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"A count of successfully transmitted frames on
         a particular interface for which transmission
         is inhibited by more than one collision."
	REFERENCE "'Intel|Ether-like|001' 5"
	::= { intelEtherLikeEntry 5 }

sqeTestErrorsAtt6 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"A count of times that the SQE TEST ERROR
	   message is generated by the PLS sublayer for a
         particular interface. The SQE TEST ERROR
         message is defined in section 7.2.2.2.4 of
         ANSI/IEEE 802.3-1985 and its generation is
         described in section 7.2.4.6 of the same
         document."
	REFERENCE "'Intel|Ether-like|001' 6"
	::= { intelEtherLikeEntry 6 }

deferredTransmissionsAtt7 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"A count of frames for which the first
         transmission attempt on a particular interface
         is delayed because the medium is busy."
	REFERENCE "'Intel|Ether-like|001' 7"
	::= { intelEtherLikeEntry 7 }

lateCollisionsAtt8 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"The number of times that a collision is
         detected on a particular interface later than
         512 bit-times into the transmission of a
         packet."
	REFERENCE "'Intel|Ether-like|001' 8"
	::= { intelEtherLikeEntry 8 }

excessiveCollisionsAtt9 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"A count of frames for which transmission on a
         particular interface fails due to excessive
         collisions."
	REFERENCE "'Intel|Ether-like|001' 9"
	::= { intelEtherLikeEntry 9 }

internalMacTransmitErrorsAtt10 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"A count of frames for which transmission on a
         particular interface fails due to an internal
         MAC sublayer transmit error."
	REFERENCE "'Intel|Ether-like|001' 10"
	::= { intelEtherLikeEntry 10 }

carrierSenseErrorsAtt11 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"The number of times that the carrier sense
         condition was lost or never asserted when
         attempting to transmit a frame on a particular
         interface."
	REFERENCE "'Intel|Ether-like|001' 11"
	::= { intelEtherLikeEntry 11 }

frameTooLongAtt12 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"A count of frames received on a particular
         interface that exceed the maximum permitted
         frame size."
	REFERENCE "'Intel|Ether-like|001' 12"
	::= { intelEtherLikeEntry 12 }

internalMacReceiveErrorsAtt13 OBJECT-TYPE
	SYNTAX		DmiCounter64
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"A count of frames for which reception on a
         particular interface fails due to an internal
         MAC sublayer receive error."
	REFERENCE "'Intel|Ether-like|001' 13"
	::= { intelEtherLikeEntry 13 }

etherChipSetAtt14 OBJECT-TYPE
	SYNTAX		DmiDisplaystring
	ACCESS		read-only
	STATUS		mandatory
	DESCRIPTION	"This object contains a description 
         Of the chipset used to realize the interface."
	REFERENCE "'Intel|Ether-like|001' 14"
	::= { intelEtherLikeEntry 14 }

END
