   5 Windows 98
 


Windows* 98 Installation Notes
==============================

LOCATION OF DRIVER:       \NT\E100BNT5.SY_ (compressed)
LOCATION OF SETUP FILE:   \NET82557.INF



Manually Adding an Adapter in Win 98
====================================

If the New Hardware Found dialog box does not appear at startup and
you cannot connect to the network, check the Device Manager list to
see if the new adapter is present. If it is not, follow these steps:

1. From the Control Panel, double-click the System icon.
2. Click the Device Manager tab.
3. Double-click Other Devices (question mark icon) in the list area.
4. Double-click PCI Ethernet Controller.
5. Click the Driver tab, then click Change Driver.
6. Select Network Adapters and click OK. 
7. Click Have Disk. Insert the PRO/100+ Server adapter disk
   and click OK.
8. Follow any prompts for Windows 98 installation disks and restart
   when prompted. 

   IMPORTANT: You must reboot after installing each adapter port.

To install PROSet software (recommended), continue to the section
"Install PROSet Software" in the Install Guide.


Hints and Tips
==============

1. If your system contains a multiport adapter and you install
   Windows 98, Windows 98 may detect the ports of the adapter as 
   82557-based adapters. If you try to upgrade the drivers for these
   adapters through the Update Drivers function of the Device Manager,
   the adapter may no longer function after rebooting.

   To resolve this problem:

   1. Double-click on the System icon in the Control Panel.
   2. Click the Device Manager tab.
   3. Highlight each port of the multiport adapter and click Remove.
   4. Shut down Windows 98, turn off the computer and unplug its power
      cord.
   5. Remove the multiport adapter card.
   6. Plug in the power cord and start Windows 98
   7. Shut down Windows 98, turn off the computer and unplug its power
      cord.
   8. Reinstall the multiport adapter card, plug in the power cord and
      start Windows 98.
      The Windows 98 OS should detect the hardware, prompting you for
      the drivers disk.

IMPORTANT: You must reboot after installing each adapter port.


2. Windows 98 Push Installation:
   
   You can find some support files and readme information in \WIN98\PUSH
   to help with Windows 98 push installations using the PRO/100+
   adapter.


*  Third-party trademarks are the property of their respective owners.
