   2 Windows NT 4.0



Windows NT* 4.0 Installation Notes
==================================

LOCATION OF DRIVER:    \NT\E100BNT.SY_ (NDIS 4.0 compressed)
                       \OEMSETUP.INF
      
      Note: NT 4.0 ships with a driver for the PRO/100B adapter.  
            However, it is recommended that you install the more recent 
            driver from the Configuration and Drivers disk.


General instructions
--------------------

After putting the adapter in the computer, you need to configure it
under Windows NT.

1  Double-click the Network icon in the Control Panel.

2  Select the Adapter tab and click Add...

3  Select Have Disk. Insert the Configuration and Drivers disk in the 
   disk drive and click OK.

4  Select "Intel EtherExpress PRO Adapter" from the list of available
   drivers and click OK.

5  The PROSet setup utility automatically scans computer resources
   and determines the settings assigned to your adapter.  It also adds a
   PROSet icon to the Control Panel for future use of PROSet.

6  (Optional) You can test the adapter by clicking the Test button.

7  To exit PROSet and finish installing the driver, click OK in the
   PROSet main menu.

8  Select the protocol(s) required (TCP/IP is the default) by selecting
   the Protocol Tab.

9  Select the network services required (by default, all are selected)
   by selecting the Service tab.

10 Click Close to continue.  Other Configuration screens may appear.
   Configure as desired.

   Note that after the driver is installed, NT may show the adapter as
   "Intel EtherExpress 82557-based 10/100 Ethernet PCI Adapter".
   PROSet will display the adapter specifically as "Intel PRO/100+ PCI
   100Base-TX, 10BaseT" adapter.  Also, the NDIS 4.0 miniport driver
   will automatically get installed in Windows NT 4.0.

11 When prompted, restart NT.

12 Repeat these steps for installing additional adapters.


Adapter Settings
================

There are two ways to run PROSet, which allows changing the adapter
settings.
   
   - From the Control Panel double-click on the PROSet icon.
   
   - From the Control Panel, double-click on the Network icon, select
     the adapters section, and double-click on the "Intel 82557-based
     10/100 Ethernet PCI adapter".


From the main PROSet menu click the Settings button to get to the
Adapter Settings screen. The defaults work correctly for most
configurations.


Network speed
-------------

Recommended setting:  Auto (default)

This parameter lets the PRO/100+ adapter know what speed to use on the 
Ethernet wire.  The choices are 10 Mbps, 100 Mbps, and Auto.
In Auto mode, the adapter detects if its environment can support 100
Mbps speed. It then sets the speed to 100 if it can, or 10 if it can't.
If you are using a cross over cable connected to another adapter, set
the speed to either 10 Mbps or 100 Mbps.
      
      Note: If you want to choose a Duplex Mode other than Auto, you
            must set the speed to either 10 Mbps or 100 Mbps.


Duplex mode
-----------

Recommended setting: Auto
      
      Auto: The adapter negotiates with the hub how to send/receive
            packets, either full or half duplex.
      
      Full duplex: The adapter sends and receives packets at the same
            time. This improves the performance of your adapter. Set
            duplex mode to full duplex only if you have a full duplex
            switch.
      
      Half duplex: The adapter performs one operation at a time. It
            either sends or receives.

      Note: To change the Duplex Mode, you must set the speed to
            either 10 Mbps or 100 Mbps.

A regular adapter can perform only one operation at a time (half-
duplexing). The PRO/100+ adapter has the ability to send and receive
packets at the same time (full-duplexing) at both 10 and 100 Mbps. In 
order to reap the benefits of full duplexing, you MUST have a full 
duplex switch.

The PRO/100+ adapter has the added ability to "talk" to the hub or
switch and determine at which mode to communicate (either full or half
duplex). This is called auto-negotiation. You must have an auto-
negotiating switch to get full duplex support with the Duplex Mode set
to Auto. If you don't have an auto-negotiating hub or switch and want to
run at full duplex, set Duplex Mode to Full and then set the SPEED 
parameter to either 100 Mbps or 10 Mbps.

      Note: To change the Duplex Mode, you must set the speed to
            either 10 Mbps or 100 Mbps.


Advanced Adapter Settings
=========================

Click the Advanced button in the Adapter Settings screen to change the
Advanced setting.
      
      Note: The defaults work correctly for most configurations. Please
            use caution when changing these parameters. Use the online
            help for additional information.


Coalesce buffers
----------------

Recommended setting:  8


Receive buffers
---------------

Recommended setting:  32


Transmit control blocks
-----------------------

Recommended setting:  16


Adaptive transmit threshold
---------------------------

Recommended setting:  On

This parameter dynamically optimizes the point at which early transmit
cycles will be executed.  This results in higher performance but may
generate an occasional underrun. To eliminate underruns, set it to OFF.


Adaptive Technology
-------------------

Recommended setting:  On

Adaptive Technology customizes the PRO/100+ adapter to the respective
operating system by downloading microcode to the silicon.  This improves
performance and minimizes CPU utilization.


Map Registers
-------------

Recommended settings: 64






*  Third-party trademarks are the property of their respective owners.
