;; Windows for Workgroups 3.11
;; OEMSETUP.INF for Intel 82557-based Ethernet PCI Adapters
;; $Revision: 7 $
[data]
type=network
version="3.11.202"
[disks]
y = \wfw,  "Intel EtherExpress PRO PCI Adapter driver disk", D100DISK
z = \ndis, "Intel EtherExpress PRO PCI Adapter driver disk", D100DISK
[netcard]
in$e100b_g="Intel EtherExpress PRO PCI Adapter (10/100)",0,ndis,ethernet,0x7,in$e100b_install,in$e100b_nif
in$e100b_T="Intel EtherExpress PRO/10+ PCI Adapter",0,ndis,ethernet,0x7,in$e100b_install,in$e100b_10_nif
[in$e100b_install]
ndis2=z:e100b.dos
ndis3=y:e100b.386
mlid=*:e100bodi.com
[in$e100b_nif]
DriverName=E100B$
param=SPEED,"Line Speed (Mbits/sec)",text,"Auto-Speed,10,100",Auto-Speed,0x30
param=FORCEDUPLEX,"Force Duplex Setting",enum,"Auto-Negotiate,0,Half-Duplex,1,Full-Duplex,2",0,0x30
[in$e100b_10_nif]
DriverName=E100B$
param=FORCEDUPLEX,"Force Duplex Setting",enum,"Half-Duplex,1,Full-Duplex,2",1,0x30
