   Hardware specifications



Hardware Specifications
=======================

System compatibility
--------------------

PCI systems


Media (cable) connectors and wiring
-----------------------------------

RJ45

Use Category 5 cabling at 100 Mbps

Supports 100BASE TX Fast Ethernet standard


Data Rate mode
--------------

10 or 100 Mbps


Interrupt levels
----------------

PCI:   INTA


SRAM Transmit/Receive Buffer
----------------------------

16 Kbytes


Power requirements
------------------

2.4 Watts @ +5VDC


Isolation voltage
-----------------

200V RMS


Operating temperature
---------------------

0 - 55 degrees C


Humidity
--------

10% - 90% non-condensing


Diagnostic LED
--------------

Activity and Link

100 Mbps


Diagnostic software
-------------------

On-board

On-network

Responder







*  Third-party trademarks are the property of their
   respective owners.
